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1)      The race vehicle and the chase vehicle and any support equipment shall exhibit no unsafe characteristics when inspected in a static state by the race organization inspectors.  This includes no leaking of oil, fuel, brake fluid, etc.  This includes no loose parts that may fall off or be thrown off during operation.
2)      The E-Stop system shall be demonstrated to be capable of pausing, re-starting and disabling the race vehicle when activated by personnel in the chase vehicle.   
3)      The E-Stop system shall be demonstrated to be capable of disabling the race vehicle when activated by personnel operating one of four push button switches on the sides and front and back of the race vehicle.  
4)      The E-Stop system shall be demonstrated to be capable of automatically disabling the race vehicle if the chase vehicle becomes more than 500 feet from the race vehicle. 
5)      The race vehicle shall sound a klaxon and show a flashing beacon when it is in a state where it is running or could be caused to run.
6)      All active sensors (laser, radar, etc) shall be certified by a qualified source to be safe to humans.
7)      The race vehicle and chase vehicle shall be ready to start the race within 5 minutes of the vehicles being positioned at the start line. (note: the race organization will not supply a GPS track for the race vehicle to follow.  The race team will be provided with a time to map the race course if they wish).
8)      Racers will leave the starting line at approximately 10 minute intervals.  Race staring position will be determined by the vehicle
s time to complete a 1 mile portion of the Pikes Peak highway on the day before the race. 
9)      The race vehicle shall obey speed limits imposed by the race organization in order to ensure safety of the personnel in the chase vehicle.  The speed limits will be communicated to the race team two weeks before the race.
10)     The race vehicle shall be programmed to stop within 100 feet after crossing the finish line and then shall be moved to a parking place under manual control.

